Install the slider and cable assembly in the reverse order of removal, and note these items: Damaged parts should be replaced. Apply multipurpose grease to the glass bracket (A) and guide rail portion of the frame (B) indicated by the arrows. Before reinstalling the motor, make sure both link lifters are parallel, and in the fully closed position. Before reinstalling the motor, install the frame and glass, then check the opening drag. |