NOTE: Take care not to damage, wrinkle or twist the carpet. Be careful not to damage the interior trim places. Remove these items: Front cargo floor Rear seat belt center anchor covers Remove the clips. Pull the rear floor carpet (A) out from both rear side trim panels (B) and rear seat slide linkage covers (C), then remove it. Install the carpet in the reverse order of removal, and note these items: Replace any damaged clips. Slip the trunk floor mat under each panel and cover properly. |