Maintenance Schedule for Normal Conditions - European Models
120,000km(6year)

Follow the Normal Conditions Maintenance Schedule if the severe driving conditions specified in the Severe Conditions Maintenance Schedule do not apply.

Service at the indicated distance or time whichever comes first

| Replace engine oil

| Replace engine oil filter

| Inspect front and rear brakes
|  | Check the brake pad and disc thickness. Check for damage or cracks front pad , front disc , rear pad , rear disc
|  | Check the brake linings for cracking, grazing, wear, and contamination
|  | Check the calipers for damage, leaks, and tightness

| Check parking brake adjustment

| Check lights alignment
Check the position of the headlights

| Test drive
Check for road stability, noise, vibration, and dashboard operation

| Inspect drive belt
Check for cracks, damage, deflection, and tension

| Replace dust and pollen filter
Replace every 20,000 km (12,500 miles) or 1 year when the customer drives primarily in urban areas that have high concentration of soot in the air, under dusty condition, or the air flow from the heating and cooling system control system becomes less than normal.

| Replace fuel filter

| Inspect idle speed

| Check expiry date for temporary repair kit bottle

Visually inspect the following items:
|  | Check for correct installation and position, check for cracks, deterioration, rust, and leaks
|  | Check tightness of screws, nuts, and joints. If necessary, retighten

| Tie-rod ends, steering gearbox, and boots
Check rack grease and steering linkage. Check the boot for damage and leaking grease

| Suspension components
|  | Check the bolts for tightness
|  | Check all dust cover for deterioration and damage

| Driveshaft boots
|  | Check the boot and boot band for cracks
|  | Check rack grease

| Brake hoses and lines (including ABS/VSA)
Check the master cylinder and ABS/VSA modulator- control unit and leakage

| All fluid levels and condition of fluids
Check levels and check for leaks. If necessary, add engine coolant , MTF , ATF, brake fluid, and windshield fluid

| Exhaust system
Check the exhaust pipe and muffler for damage, leaks, and tightness K20Z2 engine , K24A3 engine

| Fuel lines and connections
Check fuel lines for loose connections, cracks, and deterioration. Retighten loose connections and replace any damaged parts

| Tyre condition
Check for pressure, puncture, cuts, and irregular thread wear

Every 40,000 km (25,000 miles)

| Replace air cleaner element

| Replace spark plugs K20Z2 engine, K24A3 engine

| Inspect the valve clearance

Every 120,000 km (75,000 miles)

| Replace spark plugs K20Z2 engine, K24A3 engine

Every 120,000 km (75,000 miles) or 8 years

| Replace manual transmission fluid
Use genuine Honda MTF

At 120,000 km (75,000 miles) or 8 years, then every 80,000 km (50,000 miles) or 4 years

| Replace automatic transmission fluid
Use genuine Honda ATF-Z1 K20Z2 engine, K24A3 engine

At 200,000 km (120,000 miles) or 10 years, then every 100,000 km (60,000 miles) or 5 years

| Replace engine coolant
Use genuine Honda All Season Antifreeze/Coolant Type 2

Every 3 years

| Replace brake fluid
|  | Use only DOT 3 or DOT 4 brake fluid. We recommend genuine Honda Brake Fluid
|  | Check that brake fluid level is between upper and lower marks on the reservoir

Every year

| Inspect vehicle corrosion:
refer to the Body Repair Manual
|  | External Paintwork and panel Corrosion Check
|  | Under body Corrosion Check