1. Attach the upper rubber dam (A), lower side rubber dam (B), and clips (C) with adhesive tape to the inside face of the windshield (D) as shown: Be sure the rubber dam and clips line up with the alignment marks (E). Be careful not to touch the windshield where adhesive will be applied.
   Rubber dams adhesive tape:
   | Thickness 0.16 mm (0.0063 in.) Width 3.5 mm (0.14 in.)
   Clips adhesive tape:
   | Thickness 0.4 mm (0.016 in.) Width 10 mm (0.39 in.)