Low Fuel Indicator Test

Do the gauge drive circuit check. If the low fuel indicator flashes, go to Step 2 . If the low fuel indicator does not flush, replace the gauge control module assembly. Perform the multiplex integrated control system troubleshooting test mode A. If any DTC's are indicated, do the indicated DTC's troubleshooting. If no DTC's are indicated, go to Step 3 . Do the fuel gauge sending unit test. |