NOTE: Do not spill brake fluid on the vehicle; it may damage the paint; if brake fluid gets on the paint, wash it off immediately with water. Remove the access panel (A) on the driver's side. Remove the brake booster vacuum hose (B) from the clamp. For LHD model, remove the cable (C) from the body and strut bar (D). For RHD model, remove the throttle cable (E) and the A/C lines (F) from the clamp (G). Remove the strut bar on the driver's side. Remove the reservoir cap and brake fluid from the master cylinder reservoir with a syringe. | LHD model RHD model