1. If you feel too much or too little drag, loosen the locknut with the special tools, and turn the adjusting screw until the drag on the feeler gauge is correct. Tighten the locknut to the specified torque and recheck the clearance. Repeat the adjustment if necessary. Specified Torque
   K20A6 Engine:
   Intake: | 20 N·m (2.0 kgf·m, 14 lbf·ft)
   Exhaust: | 14 N·m (1.4 kgf·m, 10 lbf·ft)
   K24A3 Engine: | 20 N·m (2.0 kgf·m, 14 lbf·ft)