Install the oil filler plug (A) with a new washer (B). Install the resonator chamber. Install the intake air cover. Install the battery base, then install the ground cable. Install the air cleaner housing. Install the battery. Connect the positive (+) cable first, then the negative (−) cable to the battery. Enter the anti-theft codes for the radio and navigation system, then enter the customer's radio station presets. Do the power window control unit reset procedure. Install the splash shield. |