If the A/C compressor is marginally operable, run the engine at idle speed, and let the air conditioning work for a few minutes, then shut the engine off. Make sure you have the anti-theft code for the radio and the navigation system, then write down the frequencies for the radio′s preset buttons. Disconnect the negative cable from the battery. Recover the refrigerant with a recovery/recycling/charging station. Remove the drive belt . Remove the A/C compressor clutch connector (A) from the A/C condenser fan shroud (B). Disconnect the A/C condenser fan connector (C), then remove the wire harness clip (D) from the A/C condenser fan shroud. Remove the hose (E) from the reserve tank (F). Be careful not to damage the radiator fins when removing the A/C condenser fan shroud. |