Power Window Passenger's Motor Test

Front Passenger's Remove the passenger's door panel. Disconnect the 6P connector from the window motor. |

Test the motor by connecting battery power and ground according to the table. When the motor stops running, disconnect one lead immediately. If the motor does not run or fails to run smoothly, replace it. |

Rear Remove the rear door panel. Disconnect the 6P connector from the window motor. |

Test the motor by connecting battery power and ground according to the table. When the motor stops running, disconnect one lead immediately. If the motor does not run or fails to run smoothly, replace it. |