Make sure you have the anti-theft codes for the radio, and the navigation system, then write down the customer's radio station presets. Disconnect the negative cable from the battery, then disconnect the positive cable. Remove the intake manifold. Disconnect the starter cable (A) from the B terminal, then disconnect the BLK/WHT wire (B) from the S terminal. Remove the harness clamp (C). Remove the harness holder (D). Remove the two bolts holding the starter, then remove the starter. | DENSO: MITSUBA: MITSUBISHI: