1. Remove the shift solenoid harness connector. Measure ATF temperature sensor resistance between shift solenoid harness connector terminals No. 6 and No. 7.
   Standard: | 50 Ω−25 kΩ
If the resistance is out of standard, replace the ATF temperature sensor and solenoid harness; go to Step 17 . The ATF temperature sensor is not available separately from the solenoid harness. If the measurement is within the standard, install the removed parts; go to Step 20 . Disconnect the connectors from the shift solenoid valves. |