Clean the inlet opening (A) of the ATF strainer (B) thoroughly with compressed air, then check that it is in good condition and that the inlet opening is not clogged. Test the ATF strainer by pouring clean ATF through the inlet opening, and replace it if it is clogged or damaged. Remove the O-rings (V) (W) from the stator shaft and ATF strainer. Install the new ones when installing the valve bodies. |