DTC 5: Open In The Motor Wire Harness Turn the ignition switch ON (II). Clear the DTC with the HDS. Start the engine. Turn the steering wheel to right or left, and wait 10 seconds or more. Does the EPS indicator come on?
YES | - | Go to Step 5 .
NO | - | The system is OK at this time.■
Stop the engine, and verify the DTC. Is DTC 5 indicated?
YES | - | Go to Step 6 .
NO | - | Perform the appropriate troubleshooting for the code indicated.■
Turn the ignition switch OFF. Check the No. 22 (EPS) (70 A) fuse in the under-hood fuse/relay box, and reinstall the fuse if it is OK. Is the fuse OK?
YES | - | Go to Step 8 .
NO | - | Replace the fuse and recheck.■
Disconnect EPS control unit connector B (2P). Measure the voltage between EPS control unit connector B (2P) terminal No. 1 and body ground. Is there battery voltage?
YES | - | Go to Step 10 .
NO | - | Repair open in the wire between the No. 22 (EPS) (70 A) fuse and EPS control unit.■