Install the engine cover. Install the battery. Clean the battery posts and cable terminals with sandpaper, then assemble them and apply grease to prevent corrosion. Check that the transmission shifts into gear smoothly. Refill the engine with engine oil. Refill the transmission with fluid. Do the fuel system bleed procedure. Refill the radiator with engine coolant, and bleed air from the cooling system with the heater valve open. Do the ECM reset procedure. Do the power window control unit reset procedure. Inspect the idle speed. Enter the anti-theft codes for the radio and the navigation system, then enter the customer's radio station presets. Set the clock. |