Transmission Mount Replacement - Upper

Support the engine with a jack and wood block under the oil pan. Remove the air cleaner housing. Remove the transmission upper mount bracket. |

Remove the transmission upper mount (A). Install the new transmission upper mount, then loosely tighten the new nuts (B), and loosely tighten the new bolt (C). |

Install the transmission upper mount bracket (A), and tighten the new bolts, then loosely tighten the mounting bolt (B). Remove a jack. |

Tighten the transmission upper mount/bracket mounting bolts/nuts in the numbered sequence shown. Install the air cleaner housing. |