Remove the locknut (A) and the fuel pump/sender assembly. Remove the fuel filter (B), the fuel gauge sending unit (C), the case (D), the wire harness (E), and the fuel pressure regulator (F). When connecting the fuel pump assembly, make sure the connection is secure and the suction filter (G) is firmly connected to the fuel pump (H). Check these items before installing the fuel tank unit: When connecting the wire harness, make sure the connection is secure and the connectors (I) are firmly locked into place. When installing the fuel gauge sending unit, make sure the connection is secure and the connector is firmly locked into place. Be careful not to bend or twist it excessively. Install the parts in the reverse order of removal with a new base gasket (J), locknut and new O-rings (K). When installing the fuel tank unit, align the marks (L) on the unit (M) and the fuel tank (N). |