DTC 11-3x (11-30 to 11-39, 11-3A to 11-3F): Short to Another Wire or Decreased Resistance in Driver's Airbag Inflator (LHD) Special Tools Required SRS inflator simulator 07SAZ-TB4011A SRS simulator lead C 07TAZ-SZ5011A SRS simulator lead F 07XAZ-SZ30100 SRS short canceller 070AZ-SAA0100 Erase the DTC memory. Turn the ignition switch ON (II), and check that the SRS indicator comes on for about 6 seconds and then goes off. Does the SRS indicator stay on and is DTC 11-3x indicated?
YES | - | Go to Step 3 .
NO | - | Intermittent failure, system is OK at this time. Go to Troubleshooting Intermittent Failures. If another DTC is indicated, go to the DTC troubleshooting index for troubleshooting details.
Turn the ignition switch OFF. Disconnect the battery negative cable, and wait for 3 minutes. Disconnect the driver's airbag 2P connector (A) from the cable reel. Connect the SRS inflator simulator (2 Ω connector) and simulator lead C to the cable reel. Reconnect the battery negative cable. Erase the DTC memory. Read the DTC. Is DTC 11-3x indicated?
YES | - | Go to Step 9 .
NO | - | Short in the driver's airbag; replace the driver's airbag. ■
Turn the ignition switch OFF. Disconnect the battery negative cable, and wait for 3 minutes. |