Install the torsion bars in the reverse order of removal, and note these items: The shapes of the right torsion bar (A) and left torsion bar (B) are shown. Install the torsion bars properly. Adjust the torsion bars forward or rearward with the torsion bar assembly tool. Positions where each torsion bar was installed in the factory are: Left torsion bar: Normal position Right torsion bar: Higher tension Make sure the trunk lid opens properly and locks securely. |