DTC 112: Internal Power Source Stuck OFF NOTE: If the battery cable was disconnected three times with the ignition switch ON (II), this DTC may be stored. Check for other DTCs. Is another DTC indicated?
YES | - | Do the appropriate troubleshooting for the DTC.■
NO | - | Go to Step 2 .
Clear the DTC using the HDS. Disconnect the HDS from the 16P DLC. Turn the ignition switch OFF, then turn it ON (II) again. Test-drive the vehicle. Does the ABS indicator come on, and is DTC 112 indicated?
YES | - | Go to Step 6 .
NO | - | Intermittent failure; the vehicle is OK at this time.■
Inspect G203 for a clean and tight connection. Is G203 clean and properly connected?
YES | - | Go to Step 7 .
NO | - | Repair the connection at G203.■
Disconnect the VSA control unit 47P connector. Check for continuity between body ground and VSA control unit 47P connector terminals No. 32 and No. 47 individually. Is there continuity?
YES | - | Check for loose terminals in the VSA control unit 47P connector. If necessary, substitute a known-good VSA modulator-control unit, and recheck.■
NO | - | Repair open in the wire between the VSA modulator-control unit and G203.■