1. NOTE: Take care not to scratch the rear bumper and body. Put on gloves to prevent damage. Remove the rear bumper skirt trim (A) from the rear bumper (B).
   -1. | Remove the bolts (C, D) and clips (E) from the rear bumper.
   -2. | Remove the nuts (F), then remove the rear bumper skirt trim.
Install in the reverse order of removal, and note these items: Check the clips for damage or stress-whitening, and if necessary, replace them with new ones. Push the clips and hooks into place securely.