Used engine oil may cause skin cancer if repeatedly left in contact with the skin for prolonged periods. Although this is unlikely unless you handle used oil on a daily basis, it is still advisable to thoroughly wash your hands with soap and water as soon as possible after handling used oil.
For the details of lubrication points and type of lubricants to be applied, refer to the illustrated index and various work procedures (such as Assembly/Reassembly, Replacement, Overhaul, Installation, etc.) contained in each section.
Application | Lubricant or Fluid
--- | ---
A | Engine (european models) | Always use genuine Honda Motor Oil, ACEA A1/B1, ACEA A3/B3, or ACEA A5/B5. SAE viscosity: See chart.
Engine (except european models) | Always use API service grade SL or higher SAE viscosity: See chart.
B | Manual transmission | Honda Manual Transmission Fluid (MTF) Always use genuine Honda MTF * . Using motor oil can cause stiffer shifting because it does not contain the proper additives.
Automatic transmission | Honda ATF-Z1 Always use genuine Honda ATF-Z1. Using a non-Honda ATF can affect shift quality.
C | Brake system (including ABS/VSA lines) | Brake Fluid DOT 3 or DOT 4 We recommend genuine Honda Brake Fluid. Using a non-Honda brake fluid can cause corrosion and decrease the life of the system.
D | Clutch system (manual transmission)
E | Power steering system (power steering type) | Honda Power Steering Fluid Always use genuine Honda Power Steering Fluid. Using any other type of power steering fluid or automatic transmission fluid can cause increased wear and poor steering in cold weather.
F G H I J K L M N | Release fork (manual transmission) Battery terminals Brake booster clevis Clutch master cylinder clevis (manual transmission) Shift lever (manual transmission) Fuel fill door Hood hinges and hood latch Trunk hinges Door checker | Multipurpose Grease
O | Brake caliper piston seals | Rubber Grease
P Q | Brake caliper piston boots, piston pins and boots Shift cable ends (manual transmission) | Silicone Grease
R | Air conditioning compressor | Compressor Oil: SP-10 (P/N 38897-P13-003, 38898-P13-003, or 38899-P13-A01) For refrigerant HFC-134a (R-134a)
S | Cooling system | Honda All Season Antifreeze/Coolant Type 2
| If genuine Honda MTF is not available, use API service SL or higher grade motor oil with a viscosity of SAE 10W-30 or 10W-40 as a temporary replacement.