SRS components are located in this are. Review the SRS component locations and the precautions and procedures before performing repairs or service. NOTE: Use the handy remover set, or equivalent when prying components. When using a flat-tip screwdriver, wrap it with protective tape to prevent damage. Take care not to bend and scratch the headliner. Be careful not to damage the dashboard and other interior trim. Remove these items: Front pillar trim, both sides Ceiling light Front seat belt upper anchor, both sides Center pillar lower trim Center pillar upper trim, both sides Roof end trim Quarter pillar trim, both sides From both sides, using a handy remover, release the tabs (A), then remove the sunvisor cap (B) from the bracket (C). Turn the cap, and remove it. |