Special Tools Required Ball joint remover, 28 mm 07MAC-SL00200 Loosen the wheel nuts slightly. Raise the front of the vehicle, and support it with safety stands in the proper locations. Remove the wheel nuts and front wheels. Lift up the locking tab (A) on the spindle nut (B), then remove the nut. Drain the transmission fluid. Reinstall the drain plug using a new washer: Manual transmission Automatic transmission |