1. Remove the door panel (A) with as little bending as possible to avoid creasing or breaking it.
   -1. | Starting at the bottom edge of the door panel, release the clips (B) that are just above the marks (C) on the edge of the panel with a commercially available trim pad remover (D).
   -2. | Detach the upper clips (E, F).
   -3. | Starting at the rear, pull the door panel upward and over the lock knob (G). NOTE: The inner handle cable (H) is connected to the inner handle (I). Do not pull the door panel up too far, or the inner handle cable will be damaged.