1. NOTE: When measuring the front wheel runout, turn the other side of the wheel slowly by hand. Raise the vehicle, and support it with safety stands in the proper locations. Check for a bent or deformed wheel. Set up the dial gauge as shown, and measure the axial runout by turning the wheel.
   Front and rear wheel axial runout:
   | Standard:
   | Aluminum wheel: | 0−0.7 mm (0−0.03 in.)
   | Steel wheel: | 0−1.0 mm (0−0.04 in.)
   | Service limit: | 2.0 mm (0.08 in.)