NOTE: Do not use this troubleshooting procedure if the fans are also inoperative, or if the A/C compressor is inoperative. Refer to the symptom troubleshooting index. Check the No. 30 (7.5 A) fuse in the under-dash fuse/relay box. Is the fuse OK?
YES | - | Go to Step 2 .
NO | - | Replace the fuse, and recheck.■
Disconnect the magnet valve 2P connector. Turn the ignition switch ON (II). Measure the voltage between the No. 2 terminal of the magnet valve 2P connector and body ground. Is there battery voltage?
YES | - | Go to Step 5 .
NO | - | Repair open in the wire between the No. 30 fuse in the under-dash fuse/relay box and the magnet valve.■
Turn the ignition switch OFF. Reconnect the magnet valve 2P connector. |