Check for continuity between A/T clutch pressure control solenoid valve B connector terminal No. 2 and body ground. Is there continuity?
YES | - | Update the PCM if it does not have the latest software, or substitute a known-good PCM, then recheck. If the symptom/indication goes away with a known-good PCM, replace the original PCM .■
NO | - | Repair open in the wire between the A/T clutch pressure control solenoid valve B and ground (G101), or repair poor ground (G101), then go to Step 10 .
Clear the DTC with the HDS. Test-drive the vehicle for several minutes in the D position in all five gears. Monitor the OBD status for P0967 in the DTCs/Freeze Data in A/T Mode Menu for a pass/fail. Does the result indicate a pass?
YES | - | The problem has been corrected.■
NO | - | Return to Step 1 and recheck.■