M/T Reverse Shift Lever Clearance Inspection

1. Measure the clearance between the reverse shift lever (A) and reverse shift fork (B) with a feeler gauge (C). If the clearance is more than the service limit, go to Step 2 .
   Standard: | 0.05−0.50 mm (0.002−0.020 in.)
   Service Limit: | 0.6 mm (0.024 in.)

1. Measure the width of the reverse shift lever. If the width is not within the standard, replace the reverse shift lever. If the width is within the standard, replace the reverse shift fork.
   Standard: | 6.400−6.650 mm (0.2520−0.2618 in.)

1. Measure the clearance between the reverse shift lever (A) and reverse shift piece (B) with a feeler gauge (C). If the clearance is more than the service limit, go to Step 4 .
   Standard: | 0−0.4 mm (0−0.015 in.)
   Service Limit: | 0.5 mm (0.020 in.)

1. Measure the width of the reverse shift lever. If the width is not within the standard, replace the reverse shift lever. If the width is within the standard, replace the reverse shift piece.
   Standard: | 13.0−13.2 mm (0.51−0.52 in.)