M/T Reverse Lockout Solenoid Assembly Disassembly/Reassembly

Make sure you have the anti-theft codes for the audio and the navigation system, then write down the customer's audio presets. Disconnect the negative (−) cable first, then the positive (+) cable from the battery. Remove the battery. Remove the air cleaner housing. Remove the intake air cover. |

Remove the resonator chamber. Transmission is supported from the bottom with a jack. |

Remove the transmission mount bolt (A), nuts (B), bolt (C), and the ground cable bolt (D). |

Remove the stud bolts (A). Remove the transmission mount (B). Disconnect the reverse lockout solenoid connector. |

Remove the bolts (A), reverse lockout solenoid assembly (B). Install in the reverse order of removal. |