Install the cover in the reverse order of removal, and note these items: Check the mounting holes in the back of the seat-back frame, for the clips on the seat-back top cover, for damage before reinstallation. If necessary, make them even. To prevent wrinkles, make sure the material is stretched evenly over the pad before securing the clips. Replace any clips (A) you removed with new ones. Install them with commercially available upholstery ring pliers (B). |