SRS components are located in this area. Review the SRS component locations LHD, SRS component locations RHD and the precautions and procedures before performing repairs or service. NOTE: Use the handy remover set, or equivalent when prying components. Take care not to bend or scratch the headliner. Be careful not to damage the dashboard and other interior trim. Remove these items: Front pillar trim, both sides, without side curtain airbag, with side curtain airbag Ceiling light Front seat belt upper anchor, both sides Center pillar lower trim, without side curtain airbags, with side curtain airbags Center pillar upper trim, both sides, without side curtain airbags, with side curtain airbags Rear pillar trim, both sides, without side curtain airbags, with side curtain airbags From both sides, using a flat-tip screwdriver, release the tabs (A), then remove the sunvisor cap (B) from the bracket (C). Turn the cap, and remove it. |