Check for continuity between ECM/PCM connector terminal B19 and throttle actuator control module 16P connector terminal No. 6. Is there continuity?
YES | - | Substitute a known-good throttle actuator control module, then go to Step 50 and recheck. If DTC U0107 is not indicated, replace the original throttle actuator control module, then go to Step 50 . If DTC U0107 is indicated, go to Step 56 .
NO | - | Repair open in the wire between the ECM/PCM (B19) and the throttle actuator control module, then go to Step 50 .
Turn the ignition switch OFF. Jump the SCS line with the HDS. Disconnect the throttle actuator control module 16P connector. Disconnect ECM/PCM connector B (24P). |