B-CAN System Diagnosis Test Mode 1 (Troubleshooting without the HDS) Check the No. 9 (10 A) fuse and No. 21 (7.5 A) fuse in the under-dash fuse/relay box. Are the fuses OK?
YES | - | Go to Step 2 .
NO | - | Find and repair the cause of the blown fuse.■
Check self-diagnosis function Mode 1 for a diagnostic trouble code (DTC). If there is a DTC, the will blink, pause, then repeat the DTC as long as the ignition switch ON (II). Is there a repeating DTC?
YES | - | Count the blinks, then go to Step 4 .
NO | - | Go to Step 5 .
1. About 1 second after you go into self-diagnosis Mode 1, the ceiling light will indicate the DTC, and repeat it every 3 seconds. If there is more than one DTC, the system will indicate them in ascending order, beginning from the DTC with the lowest numerical value. Troubleshoot the DTCs as indicated: DTC 2, 3, 4 and 5 simultaneously: Check for an open in the BLU wire between multiplex integrated control unit D11 and relay module J7, BRN/RED wire between multiplex integrated control unit J4 and door multiplex control unit No. 16, LT BLU wire between multiplex integrated control unit X27 and combination switch control unit No. 4, WHT wire between multiplex integrated control unit N28 and gauge B25. If the wire is OK, substitute a known-good under-dash fuse/relay box (multiplex integrated control unit), under-hood fuse/relay box, power window master switch, wiper/washer switch and gauge one at a time, in that order, and recheck for the DTCs after each substitution. DTC 1 only go to MICU input test. DTC 2 only (no other DTCs present): Go to the relay module input test. If all inputs are OK, substitute a known-good relay module and then a MICU, one at a time, and then check for DTCs. If a DTC recurs after a substitution, replace that unit. DTC 3 only (no other DTCs present): Go to the door multiplex control unit input test. If all inputs are OK, substitute a known-good door multiplex control unit and then a MICU, one at a time, and then check for DTCs. If a DTC recurs after a substitution, replace that unit. DTC 4 only (no other DTCs present): Go to the combination switch control unit input test. If all inputs are OK, substitute a known-good wiper/washer switch and then a MICU, one at a time, and then check for DTCs. If a DTC recurs after a substitution, replace that unit. DTC 5 only (no other DTCs present): Go to the gauge control module input test. If all inputs are OK, substitute a known-good gauge control module and then a MICU, one at a time, and then check for DTCs. If a DTC recurs after a substitution, replace that unit.
   DTC | Cause
   --- | ---
   1 | The MICU cannot receive signals from the BUS communication line.
   2 | The MICU cannot receive signals from the relay module communication line.
   3 | The MICU cannot receive signals from the power window communication line.
   4 | The MICU cannot receive signal from the combination switch communication line.
   5 | The MICU cannot receive signals from the gauge control module.
1. Switch the MICS to Mode 2. Look in the following table for the switches most closely related to the problem then operate that switch. If the circuit is OK, the ceiling light should blink once. If the circuit is faulty, there will be no indication. In the table is a list of circuits that can be checked in Mode 2. Unit: MICU
   Item
   Driver's door switch
   Front passenger's door switch
   Left rear door switch
   Right rear door switch
   Trunk latch switch
   Front passenger's door lock knob switch (UNLOCK)
   Left rear door lock knob switch (UNLOCK)
   Right rear door lock knob switch (UNLOCK)
   Ignition key switch
   Audio-HVAC-display module security ground (disconnected)
   Driver's seat belt switch (unbuckled)
   Brake pedal position switch
   Unit: RELAY CONTROL MODULE
   Item
   Windshield wiper switch (motor park)
   Hood switch
   A/C pressure switch
   Unit: COMBINATION SWITCH CONTROL UNIT
   Item
   Turn signal switch (LEFT)
   Turn signal switch (RIGHT)
   Combination light switch
   Dimmer switch
   Passing switch
   Windshield wiper switch
   Intermittent dwell time controller
   Windshield washer switch
   Unit: POWER WINDOW MASTER SWITCH (DOOR MULTIPLEX CONTROL UNIT
   Item
   Power window master switch (DRIVER'S MANUAL UP)
   Power window master switch (DRIVER'S MANUAL DOWN)
   Power window master switch (DRIVER'S AUTO UP)
   Power window master switch (DRIVER'S AUTO DOWN)
   Power window master switch (FRONT PASSENGER'S UP)
   Power window master switch (FRONT PASSENGER'S DOWN)
   Power window master switch (LEFT REAR UP)
   Power window master switch (LEFT REAR DOWN)
   Power window master switch (RIGHT REAR UP)
   Power window master switch (RIGHT REAR DOWN)
   Driver's door key cylinder switch (LOCK)
   Driver's door key cylinder switch (UNLOCK)
   Driver's door lock switch (LOCK)
   Driver's door lock switch (UNLOCK)
   Driver's door lock knob switch (LOCK)
   Driver's door lock knob switch (UNLOCK)
   Keyless receiver (LOCK)
   Keyless receiver (UNLOCK)
   Keyless receiver (TRUNK)
   Unit: GAUGE CONTROL MODULE
   Item
   Parking brake switch
   Cruise Set/Resume/Cancel switch
   Transmission range switch
   Brake fluid level switch
Does the ceiling light indicate proper switch operation?
YES | - | Go to function and input test for the system related to the failure.■
NO | - | Repair the open, short, or replace the faulty switch.■