Adaptive Cruise Control/LKAS Combination Switch Replacement

Remove the steering wheel. Remove the steering wheel rear cover (A). Remove the voice control switch (B) and the distance/LKAS off switch (C). |

Remove the adaptive cruise control (ACC)/LKAS combination switch assembly (A). Install the parts in the reverse order of removal. Do the steering angle sensor neutral position memorization procudure. |