DTC 64: Sensor Power Voltage Clear the DTC using the HDS. Test-drive the vehicle. Does the ABS indicator come on, and is DTC 64 indicated?
YES | - | Go to Step 3 .
NO | - | The system is OK at this time.■
Turn the ignition switch OFF. Disconnect the VSA control unit 47P connector and steering angle sensor 5P connector. Check for continuity between the VSA control unit 47P connector terminal No. 7 and body ground. Is there continuity?
YES | - | Repair short to body ground between the VSA modulator-control unit and steering angle sensor.■
NO | - | Replace the VSA modulator-control unit. ■