NOTE: Take care not to tear the seams or damage the seat covers. Put on gloves to protect your hands. Tilt the seat-back forward and tip the seat cushion up. Remove these items: Headrest and center headrest Cargo net (for some models) Seat-back top cover Remove the bolts (A) and nut (B), disconnect the rod (C), then remove the seat-back latch (D) from the seat-back frame. Install the latch in the reverse order of removal, and note these items: Make sure the rod is connected securely. Make sure the seat-back locks securely and unlocks properly. Make sure the headrest doesn't stand still if the seat-back was unlocked. |