NOTE: Check the rear seat belts for damage, and replace them if necessary. Be careful not to damage them during removal and installation. Rear Seat Belt Remove the rear seat side bolster. Fold the seat-back forward, then remove the lower anchor bolt (A). Recline the seat-back half-way back, then remove these items: Headrest and center headrest Cargo net (for some models) Seat-back top cover Armrest (right seat-back) Release the clips fastening the seat-back cover as needed, and unzip the cover. Remove the center headrest guides from the seat-back. Recline the seat-back fully, and secure it. Pull out the center seat belt as needed (right seat-back), then pull back the seat-back cover/pad from the frame. |