Rear Pillar Outer Trim Replacement

1. NOTE: Take care not to scratch the body. Remove the taillight. While pulling the rear pillar outer trim (A), cut through the double-sided adhesive tape (B, C) with a utility knife, then remove it. Adhesive tape
   B: | Thickness 1.6 mm (0.063 in.)
   | Width 10 mm (0.39 in.)
   C: | Thickness 2.5 mm (0.098 in.)
   | Width 10 mm (0.39 in.)
Install the rear pillar outer trim in the reverse order of removal, and note these items: If the trim is to be reinstalled, scrape off the remaining double-sided adhesive tape from the trim and body, then clean the trim and body surface with a sponge dampened in alcohol where adhesive tape will be applied. Attach the upper double-sided adhesive tape (B) and another double-sided adhesive tape (C) to the original position in the trim. Fit the pins (D) to the clips (E) on the rear pillar, then push the clips and adhesive portions into place securely. Replace any damaged clips with new ones. |