1. Marking the target position of the driver's side Measuring distance XX mm from the mark (N) described is put in Step 16 to the driver's side, and it put the mark (O) on the floor.
   Prescribed distance | Offset distance XX
   1,500 mm (59.055 in.) | 436 mm (17.165 in.)
   2,000 mm (78.74 in.) | 524 mm (20.629 in.)
   2,500 mm (98.425 in.) | 612 mm (24.094 in.)
   3,000 mm (118.11 in.) | 700 mm (27.559 in.)
NOTE: The distance XX depends on the prescribed distance X which is chosen in Step 3 . Choose the offset distance XX which corresponds to the chosen prescribed distance. |