Secondary shaft

Item | Measurement | Qualification | Standard or New | Service Limit
--- | --- | --- | --- | ---
Secondary shaft | Diameter of needle bearing contact area | At 1st gear | 39.986−39.999 mm (1.5742−1.5748 in.) | When worn or damaged
At 2nd gear | 39.986−39.999 mm (1.5742−1.5748 in.) | When worn or damaged
At 3rd gear collar | 36.975−36.991 mm (1.4557−1.4563 in.) | When worn or damaged
I.D. of gears | 1st gear | 47.000−47.016 mm (1.8504−1.8510 in.) | When worn or damaged
2nd gear | 46.000−46.016 mm (1.8110−1.8116 in.) | When worn or damaged
3rd gear | 43.000−43.016 mm (1.6929−1.6935 in.) | When worn or damaged
End play of gears | 1st gear | 0.04−0.12 mm (0.002−0.005 in.) | ———
2nd gear | 0.04−0.12 mm (0.002−0.005 in.) | ———
3rd gear | 0.10−0.22 mm (0.004−0.009 in.) | ———
37 x 58 mm thrust washer thickness | No. 1 | 3.900 mm (0.154 in.) | When worn or damaged
No. 2 | 3.925 mm (0.155 in.) | When worn or damaged
No. 3 | 3.950 mm (0.156 in.) | When worn or damaged
No. 4 | 3.975 mm (0.156 in.) | When worn or damaged
No. 5 | 4.000 mm (0.157 in.) | When worn or damaged
No. 6 | 4.025 mm (0.158 in.) | When worn or damaged
No. 7 | 4.050 mm (0.159 in.) | When worn or damaged
No. 8 | 4.075 mm (0.160 in.) | When worn or damaged
No. 9 | 4.100 mm (0.161 in.) | When worn or damaged
No. 10 | 4.125 mm (0.162 in.) | When worn or damaged
No. 11 | 4.150 mm (0.163 in.) | When worn or damaged
No. 12 | 4.175 mm (0.164 in.) | When worn or damaged
No. 13 | 4.200 mm (0.165 in.) | When worn or damaged
No. 14 | 4.225 mm (0.166 in.) | When worn or damaged
No. 15 | 4.250 mm (0.167 in.) | When worn or damaged
No. 16 | 4.275 mm (0.168 in.) | When worn or damaged
No. 17 | 4.300 mm (0.169 in.) | When worn or damaged
No. 18 | 4.325 mm (0.170 in.) | When worn or damaged
No. 19 | 4.350 mm (0.171 in.) | When worn or damaged
No. 20 | 4.375 mm (0.172 in.) | When worn or damaged
40 x 51.5 mm thrust washer thickness | No. 1 | 4.80 mm (0.189 in.) | When worn or damaged
No. 2 | 4.85 mm (0.191 in.) | When worn or damaged
No. 3 | 4.90 mm (0.193 in.) | When worn or damaged
No. 4 | 4.95 mm (0.195 in.) | When worn or damaged
No. 5 | 5.00 mm (0.197 in.) | When worn or damaged
No. 6 | 5.05 mm (0.199 in.) | When worn or damaged
3rd gear collar length |  | 43.9−44.0 mm (1.728−1.732 in.) | ———
Length of 3rd gear collar flange from end |  | 5.25−5.40 mm (0.207−0.213 in.) | When worn or damaged
Sealing ring thickness |  | 1.91−1.97 mm (0.0752−0.0776 in.) | 1.86 mm (0.0732 in.)
Width of sealing ring groove |  | 2.025−2.060 mm (0.0797−0.0811 in.) | 2.080 mm (0.0819 in.)
Clutch feed pipe O.D. | 3rd clutch feed pipe | 11.47−11.48 mm (0.4516−0.4520 in.) | 11.45 mm (0.4508 in.)
1st clutch feed pipe | 6.97−6.98 mm (0.2744−0.2748 in.) | 6.95 mm (0.2736 in.)
Clutch feed pipe bushing O.D. | 3rd clutch feed pipe | 11.500−11.518 mm (0.4528−0.4553 in.) | 11.530 mm (0.4539 in.)
1st clutch feed pipe | 7.018−7.030 mm (0.2763−0.2768 in.) | 7.045 mm (0.2774 in.)
ATF guide of sealing ring contact I.D. |  | 29.000−29.021 mm (1.1417−1.1426 in.) | 29.05 mm (1.144 in.)