Bleed the clutch hydraulic system. Attach a hose to the bleeder screw (A), and suspend the hose in a container of brake fluid. Make sure there is an adequate supply of fluid in the clutch master cylinder, then slowly pump the clutch pedal until no more bubbles appear at the bleeder hose. It may be necessary to limit the movement of the release fork (B) with a block of wood to remove all the air from the system. Tighten the bleeder screw to 8 N·m (0.8 kgf·m, 5.8 lbf·ft); do not overtighten it. Refill the clutch master cylinder with fluid when done. Always use only Honda DOT 3 or 4 brake fluid. Install the air cleaner housing. Reconnect the battery cables; positive (+) cable first, then the negative (−) cable. Enter the anti-theft code for the radio and navigation system, then enter the customer's radio station presets. Perform the power window control unit reset procedure. |