DTC P0341: CMP Sensor and CKP Sensor Incorrect Phase Detected Turn the ignition switch ON (II). Clear the DTC with the HDS. Test-drive at a steady speed between 30−60 km/h (19−38 mph) for 10 minutes. Check for Temporary DTCs or DTCs in the DTCs MENU with the HDS. Is DTC P0341 indicated?
YES | - | Go to Step 9 .
NO | - | Go to Step 5 .
Do the VTC TEST in the INSPECTION MENU with the HDS. Is the result OK?
YES | - | Go to Step 6 .
NO | - | Go to Step 9 .
Test-drive at a steady speed between 30−60 km/h (19−38 mph) for 10 minutes. Check the VTC STATUS in the DATA LIST with the HDS. Does it indicate ON?
YES | - | Go to Step 8 .
NO | - | Go to Step 6 and recheck.
Monitor the OBD STATUS for DTC P0341 in the DTCs MENU with the HDS. Does the screen indicate FAILED?
YES | - | Go to Step 9 .
NO | - | If the screen indicates PASSED, intermittent failure, system is OK at this time. Check for poor connections or loose terminals at the VTC oil control solenoid valve and the ECM/PCM. If the screen indicates NOT COMPLETED, go to Step 6 and recheck.
Turn the ignition switch OFF. Test the VTC oil control solenoid valve. Is the VTC oil control solenoid valve OK?
YES | - | Go to Step 11 .
NO | - | Replace the VTC oil control solenoid valve, then go to Step 14 .
Check the camshaft timing. Is the camshaft timing OK?
YES | - | Go to Step 12 .
NO | - | Time the camshaft, then go to Step 14 .
Check for damage to the cam chain. Is the cam chain damaged?
YES | - | Replace the cam chain, then go to Step 14 .
NO | - | Go to Step 13 .
Inspect the VTC actuator. Is the result OK?
YES | - | Go to Step 14 .
NO | - | Replace the VTC actuator, then go to Step 14 .
Turn the ignition switch ON (II). Reset the ECM/PCM with the HDS. Clear the CKP pattern with the HDS. Do the ECM/PCM idle learn procedure. Do the CKP pattern learn procedure. Test-drive at a steady speed between 30−60 km/h (19−38 mph) for 10 minutes. Check for Temporary DTCs or DTCs in the DTCs MENU with the HDS. Are any Temporary DTCs or DTCs indicated?
YES | - | If DTC P0341 is indicated, check for poor connections or loose terminals at the VTC oil control solenoid valve and the ECM/PCM, then go to Step 1 . If any other Temporary DTCs or DTCs are indicated, go to the indicated DTC's troubleshooting.
NO | - | Go to Step 21 .
Monitor the OBD STATUS for DTC P0341 in the DTCs MENU with the HDS. Does the screen indicate PASSED?
YES | - | Troubleshooting is complete.■
NO | - | If the screen indicates FAILED, check for poor connections or loose terminals at the VTC oil control solenoid valve and the ECM/PCM, then go to Step 1 . If the screen indicates NOT COMPLETED, go to Step 19 and recheck.