1. Check for continuity between the appropriate EPS control unit connector D (3P) terminal and torque sensor 3P connector terminal (see table).
   Terminal name | Torque Sensor terminal No. | EPS control unit D terminal No.
   --- | --- | ---
   VS1 | 1 | 1
   PVF | 2 | 2
   VS2 | 3 | 3
Is there continuity?
YES | - | Go to Step 11 .
NO | - | Repair open in the wire between the appropriate torque sensor and EPS control unit.■