Crankshaft Pulley Removal and Installation

Special Tools Required Handle 07JAB-001020B Pulley holder attachment, HEX 50 mm 07JAB-0010400 Socket wrench, 19 mm 07JAA-001020A Removal Remove the right front tyre/wheel. Remove the splash shield. Hold the pulley with handle (A) and holder attachment (B). Remove the bolt with a 19 mm socket (C) and breaker bar. |

Installation Clean the crankshaft pulley (A), crankshaft (B), bolt (C), and washer (D). Lubricate the new engine oil as shown. |

Install the crankshaft pulley, and hold the pulley with handle (A) and holder attachment (B). Tighten the bolt to 29 N·m (3.0 kgf·m, 22 lbf·ft) with a torque wrench and 19 mm socket (C). Do not use an impact wrench. If you are using a new pulley bolt or new crankshaft, tighten the bolt to 34 N·m (3.5 kgf·m, 25 lbf·ft). Tighten the pulley bolt an additional 90 °. Install the splash shield. Install the right front tyre/wheel. |