ABS indicator does not come on Turn the ignition switch ON (II), and watch the ABS indicator. Does the ABS indicator come on for several seconds?
YES | - | The system is OK at this time.■
NO | - | Go to Step 2 .
Do the gauge control module self-diagnosis function procedure. Is gauge control module OK?
YES | - | Go to Step 3 .
NO | - | Replace gauge control module. ■
Turn the ignition switch OFF. Remove the gauge control module. Disconnect the gauge control module connector (36P). Cheek for continuity between gauge control module connector (36P) terminal No. 13 and the body ground. Is there continuity?
YES | - | Repair short to body ground in the wire between the gauge control module and the ABS modulator-control unit.■
NO | - | Check for loose terminals in the gauge control module connectors. If connectors are OK, replace the gauge control module .■