Maintenance Schedule for Severe Conditions
100,000km(5year)

Follow the Severe Conditions Maintenance Schedule if the customer's vehicle is driven MAINLY under one or more of the following conditions:

- Driving less than 8 km (5 miles) per trip or, in freezing temperatures, driving less than 16 km (10 miles) per trip.
- Driving in extremely hot over 35 °C (95 °F) conditions.
- Extensive idling, or long periods of stop-and-go-driving.
- Trailer towing, driving with a car-top carrier, or driving in mountainous conditions.
- Driving on muddy, dusty, or de-iced roads.

NOTE: If the customer's vehicle is driven OCCASIONALLY under severe conditions, follow the Normal Conditions Maintenance Schedule.

Service at the indicated distance or time whichever comes first

| Drain fuel filter

| Check parking brake adjustment
Check the parking brake operation

| Check lights alignment
Check the position of the headlights

| Test drive (noise, stability, dashboard operation)

| Check expirty date for IMS bottle (if equipped)

Visually inspect the following items:
|  | Check for correct installation and position, check for cracks, deterioration, rust, and leaks
|  | Check tightness of screws, nuts, and joints. If necessary, retighten

| Brake hoses and lines (including ABS or VSA)
Check the master cylinder, proportioning control valve, and ABS or VSA modulator and leakage

| All fluid levels and condition of fluids
Check levels and check for leaks. If necessary, and engine coolant, MTF , brake fluid, power steering fluid, and windshield fluid

| Exhaust system
Check the catalytic converter heat shield, exhaust pipe, and muffler for damage, leaks, and tightness

| Fuel lines and connections
Check fuel lines for loose connections, cracks, and deterioration. Retighten loose connections and replace any damaged parts

| Tyre condition

Every 10,000 km (6,250 miles) or 6 months

| Replace engine oil

| Replace engine oil filter

| Inspect front and rear brakes
|  | Check the brake pad and disc thickness. Check for damage or cracks front pad, front disc, rear pad, rear disc
|  | Check the brake linings for cracking, grazing, wear, and contamination
|  | Check the calipers for damage, leaks, and tightness

Visually inspect the following items:

| Tie-rod ends, steering gearbox, and boots
Check rack grease and steering linkage. Check the boot for damage and leaking grease

| Suspension components
|  | Check the bolts for tightness
|  | Check all dust cover for deterioration and damage

| Driveshaft boots
|  | Check the boot and boot band for cracks
|  | Check rack grease

Every 20,000 km (12,500 miles)

| Replace air cleaner element
Use normal conditions except in dusty conditions

At 100,000 km (62,500 miles) or 5 years, then every 60,000 km (37,500 miles) or 3 years

| Replace engine coolant
Use genuine Honda All Season Antifreeze/ Coolant Type 2

Every 60,000 km (37,500 miles) or 4 years

| Replace manual transmission fluid
Use Honda MTF

Every 3 years

| Replace brake fluid
|  | Use only DOT 3 or DOT 4 brake fluid. We recommend genuine Honda Brake Fluid
|  | Check that brake fluid level between the upper and lower marks on the reservoir

Every 30,000 km (18,000 miles) or 1 year

| Replace dust and pollen filter