Special Tools Required Handle driver 07749-0010000 Driver attachment, 72 x 75 mm 07746-0010600 Preload inspection tool 07HAJ-PK40201 NOTE: If the transmission housing, torque converter housing, differential carrier, carrier bearing and outer race, or thrust shim were replaced, the bearing preload must be adjusted. Coat all parts with ATF during installation. Do not use the thrust shim in the torque converter housing. Remove the bearing outer race (A), 76.2 mm thrust washer (B), and 76 mm thrust shim (C) from the transmission housing (D) by heating the housing to about 100 °C (212 °F) with a heat gun (E). Do not heat the housing more than 100 °C (212 °F). NOTE: Let the transmission housing cool to room temperature before adjusting the bearing preload. |