DTC P0713: Open in ATF Temperature Sensor Circuit NOTE: Record all freeze data and review General Troubleshooting Information before you troubleshoot. This code is caused by an electrical circuit problem and cannot be caused by a mechanical problem in the transmission. Check ATF temperature sensor voltage with the HDS in the A/T data list. Does ATF temperature sensor voltage exceed 4.93 V?
YES | - | Go to Step 2 .
NO | - | Intermittent failure, the system is OK at this time. Check for poor connections or loose terminals at the ATF temperature sensor and PCM.■
Turn the ignition switch OFF. Disconnect the shift solenoid harness connector. Turn the ignition switch ON (II). Measure the voltage between shift solenoid harness connector terminal No. 6 and body ground. Is there about 5 V?
YES | - | Go to Step 6 .
NO | - | Go to Step 7 .