Release the clip (A) from middle of the carpet (B). Release the hooks (C) with a flat-tip screwdriver by pushing the screwdriver toward the door, then lift upwards. Pull the fastener (D) out, then remove the carpet. Install the carpet in the reverse order of removal, and note these items: Take care not to damage, wrinkle or twist the carpet. Make sure the seat harnesses and antenna lead are routed correctly. Replace any damaged clips. With side curtain airbag: Reconnect the negative cable to the battery. Reset the clock. Perform the power window control unit reset procedure. |